{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Analysis & Synthesis Quartus II " "Info: Running Quartus II Analysis & Synthesis" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition " "Info: Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Mon Mar 07 11:20:32 2022 " "Info: Processing started: Mon Mar 07 11:20:32 2022" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_map --read_settings_files=on --write_settings_files=off double_selector_8b -c double_selector_8b " "Info: Command: quartus_map --read_settings_files=on --write_settings_files=off double_selector_8b -c double_selector_8b" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "ISGN_NUM_OF_DESIGN_UNITS_AND_ENTITIES" "double_selector_8b.bdf 1 1 " "Info: Found 1 design units, including 1 entities, in source file double_selector_8b.bdf" { { "Info" "ISGN_ENTITY_NAME" "1 double_selector_8b " "Info: Found entity 1: double_selector_8b" {  } { { "double_selector_8b.bdf" "" { Schematic "D:/projects/quartus/double_selector_8b/double_selector_8b.bdf" { } } }  } 0 0 "Found entity %1!d!: %2!s!" 0 0 "" 0 -1}  } {  } 0 0 "Found %2!llu! design units, including %3!llu! entities, in source file %1!s!" 0 0 "" 0 -1}
{ "Info" "ISGN_START_ELABORATION_TOP" "double_selector_8b " "Info: Elaborating entity \"double_selector_8b\" for the top level hierarchy" {  } {  } 0 0 "Elaborating entity \"%1!s!\" for the top level hierarchy" 0 0 "" 0 -1}
{ "Info" "ICUT_CUT_TM_SUMMARY" "34 " "Info: Implemented 34 device resources after synthesis - the final resource count might be different" { { "Info" "ICUT_CUT_TM_IPINS" "18 " "Info: Implemented 18 input pins" {  } {  } 0 0 "Implemented %1!d! input pins" 0 0 "" 0 -1} { "Info" "ICUT_CUT_TM_OPINS" "8 " "Info: Implemented 8 output pins" {  } {  } 0 0 "Implemented %1!d! output pins" 0 0 "" 0 -1} { "Info" "ICUT_CUT_TM_LCELLS" "8 " "Info: Implemented 8 logic cells" {  } {  } 0 0 "Implemented %1!d! logic cells" 0 0 "" 0 -1}  } {  } 0 0 "Implemented %1!d! device resources after synthesis - the final resource count might be different" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Analysis & Synthesis 0 s 0 s Quartus II " "Info: Quartus II Analysis & Synthesis was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "250 " "Info: Peak virtual memory: 250 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Mon Mar 07 11:20:33 2022 " "Info: Processing ended: Mon Mar 07 11:20:33 2022" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:01 " "Info: Elapsed time: 00:00:01" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:00 " "Info: Total CPU time (on all processors): 00:00:00" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Fitter Quartus II " "Info: Running Quartus II Fitter" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition " "Info: Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Mon Mar 07 11:20:34 2022 " "Info: Processing started: Mon Mar 07 11:20:34 2022" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_fit --read_settings_files=off --write_settings_files=off double_selector_8b -c double_selector_8b " "Info: Command: quartus_fit --read_settings_files=off --write_settings_files=off double_selector_8b -c double_selector_8b" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "IQCU_PARALLEL_AUTODETECT_MULTIPLE_PROCESSORS" "4 4 " "Info: Parallel compilation is enabled and will use 4 of the 4 processors detected" {  } {  } 0 0 "Parallel compilation is enabled and will use %1!i! of the %2!i! processors detected" 0 0 "" 0 -1}
{ "Info" "IMPP_MPP_USER_DEVICE" "double_selector_8b EP2C8Q208C8 " "Info: Selected device EP2C8Q208C8 for design \"double_selector_8b\"" {  } {  } 0 0 "Selected device %2!s! for design \"%1!s!\"" 0 0 "" 0 -1}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "Low junction temperature 0 degrees C " "Info: Low junction temperature is 0 degrees C" {  } {  } 0 0 "%1!s! is %2!s!" 0 0 "" 0 -1}
{ "Info" "ICUT_CUT_USING_OPERATING_CONDITION" "High junction temperature 85 degrees C " "Info: High junction temperature is 85 degrees C" {  } {  } 0 0 "%1!s! is %2!s!" 0 0 "" 0 -1}
{ "Info" "IFITCC_FITCC_INFO_AUTO_FIT_COMPILATION_ON" "" "Info: Fitter is performing an Auto Fit compilation, which may decrease Fitter effort to reduce compilation time" {  } {  } 0 0 "Fitter is performing an Auto Fit compilation, which may decrease Fitter effort to reduce compilation time" 0 0 "" 0 -1}
{ "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED" "" "Info: Device migration not selected. If you intend to use device migration later, you may need to change the pin assignments as they may be incompatible with other devices" { { "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED_SUB" "EP2C5Q208C8 " "Info: Device EP2C5Q208C8 is compatible" {  } {  } 2 0 "Device %1!s! is compatible" 0 0 "" 0 -1} { "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED_SUB" "EP2C5Q208I8 " "Info: Device EP2C5Q208I8 is compatible" {  } {  } 2 0 "Device %1!s! is compatible" 0 0 "" 0 -1} { "Info" "IFSAC_FSAC_MIGRATION_NOT_SELECTED_SUB" "EP2C8Q208I8 " "Info: Device EP2C8Q208I8 is compatible" {  } {  } 2 0 "Device %1!s! is compatible" 0 0 "" 0 -1}  } {  } 2 0 "Device migration not selected. If you intend to use device migration later, you may need to change the pin assignments as they may be incompatible with other devices" 0 0 "" 0 -1}
{ "Info" "IFIOMGR_RESERVED_PIN_WITH_LOCATION" "3 " "Info: Fitter converted 3 user pins into dedicated programming pins" { { "Info" "IFIOMGR_RESERVED_PIN_WITH_LOCATION_SUB" "~ASDO~ 1 " "Info: Pin ~ASDO~ is reserved at location 1" {  } { { "d:/altera/90sp2/quartus/bin/pin_planner.ppl" "" { PinPlanner "d:/altera/90sp2/quartus/bin/pin_planner.ppl" { ~ASDO~ } } } { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "" { ~ASDO~ } "NODE_NAME" } }  } 0 0 "Pin %1!s! is reserved at location %2!s!" 0 0 "" 0 -1} { "Info" "IFIOMGR_RESERVED_PIN_WITH_LOCATION_SUB" "~nCSO~ 2 " "Info: Pin ~nCSO~ is reserved at location 2" {  } { { "d:/altera/90sp2/quartus/bin/pin_planner.ppl" "" { PinPlanner "d:/altera/90sp2/quartus/bin/pin_planner.ppl" { ~nCSO~ } } } { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "" { ~nCSO~ } "NODE_NAME" } }  } 0 0 "Pin %1!s! is reserved at location %2!s!" 0 0 "" 0 -1} { "Info" "IFIOMGR_RESERVED_PIN_WITH_LOCATION_SUB" "~LVDS54p/nCEO~ 108 " "Info: Pin ~LVDS54p/nCEO~ is reserved at location 108" {  } { { "d:/altera/90sp2/quartus/bin/pin_planner.ppl" "" { PinPlanner "d:/altera/90sp2/quartus/bin/pin_planner.ppl" { ~LVDS54p/nCEO~ } } } { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "" { ~LVDS54p/nCEO~ } "NODE_NAME" } }  } 0 0 "Pin %1!s! is reserved at location %2!s!" 0 0 "" 0 -1}  } {  } 0 0 "Fitter converted %1!d! user pins into dedicated programming pins" 0 0 "" 0 -1}
{ "Info" "ITDC_FITTER_TIMING_ENGINE" "Classic " "Info: Fitter is using the Classic Timing Analyzer" {  } {  } 0 0 "Fitter is using the %1!s! Timing Analyzer" 0 0 "" 0 -1}
{ "Info" "ITAN_TDC_NO_DEFAULT_OPTIMIZATION_GOALS" "" "Info: Timing requirements not specified -- quality metrics such as performance and power consumption may be sacrificed to reduce compilation time." {  } {  } 0 0 "Timing requirements not specified -- quality metrics such as performance and power consumption may be sacrificed to reduce compilation time." 0 0 "" 0 -1}
{ "Info" "IFSAC_FSAC_REGISTER_PACKING_START_REGPACKING_INFO" "" "Info: Starting register packing" {  } {  } 0 0 "Starting register packing" 0 0 "" 0 -1}
{ "Extra Info" "IFSAC_FSAC_START_REG_LOCATION_PROCESSING" "" "Extra Info: Performing register packing on registers with non-logic cell location assignments" {  } {  } 1 0 "Performing register packing on registers with non-logic cell location assignments" 1 0 "" 0 -1}
{ "Extra Info" "IFSAC_FSAC_FINISH_REG_LOCATION_PROCESSING" "" "Extra Info: Completed register packing on registers with non-logic cell location assignments" {  } {  } 1 0 "Completed register packing on registers with non-logic cell location assignments" 1 0 "" 0 -1}
{ "Extra Info" "IFSAC_FSAC_REGISTER_PACKING_BEGIN_FAST_REGISTER_INFO" "" "Extra Info: Started Fast Input/Output/OE register processing" {  } {  } 1 0 "Started Fast Input/Output/OE register processing" 1 0 "" 0 -1}
{ "Extra Info" "IFSAC_FSAC_REGISTER_PACKING_FINISH_FAST_REGISTER_INFO" "" "Extra Info: Finished Fast Input/Output/OE register processing" {  } {  } 1 0 "Finished Fast Input/Output/OE register processing" 1 0 "" 0 -1}
{ "Extra Info" "IFSAC_FSAC_START_IO_MULT_RAM_PACKING" "" "Extra Info: Moving registers into I/O cells, Multiplier Blocks, and RAM blocks to improve timing and density" {  } {  } 1 0 "Moving registers into I/O cells, Multiplier Blocks, and RAM blocks to improve timing and density" 1 0 "" 0 -1}
{ "Extra Info" "IFSAC_FSAC_FINISH_IO_MULT_RAM_PACKING" "" "Extra Info: Finished moving registers into I/O cells, Multiplier Blocks, and RAM blocks" {  } {  } 1 0 "Finished moving registers into I/O cells, Multiplier Blocks, and RAM blocks" 1 0 "" 0 -1}
{ "Info" "IFSAC_FSAC_REGISTER_PACKING_FINISH_REGPACKING_INFO" "" "Info: Finished register packing" { { "Extra Info" "IFSAC_NO_REGISTERS_WERE_PACKED" "" "Extra Info: No registers were packed into other blocks" {  } {  } 1 0 "No registers were packed into other blocks" 0 0 "" 0 -1}  } {  } 0 0 "Finished register packing" 0 0 "" 0 -1}
{ "Info" "IFITCC_FITTER_PREPARATION_END" "00:00:00 " "Info: Fitter preparation operations ending: elapsed time is 00:00:00" {  } {  } 0 0 "Fitter preparation operations ending: elapsed time is %1!s!" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_PLACEMENT_PREP_START" "" "Info: Fitter placement preparation operations beginning" {  } {  } 0 0 "Fitter placement preparation operations beginning" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_PLACEMENT_PREP_END" "00:00:00 " "Info: Fitter placement preparation operations ending: elapsed time is 00:00:00" {  } {  } 0 0 "Fitter placement preparation operations ending: elapsed time is %1!s!" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_PLACEMENT_START" "" "Info: Fitter placement operations beginning" {  } {  } 0 0 "Fitter placement operations beginning" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_INFO_VPR_PLACEMENT_FINISH" "" "Info: Fitter placement was successful" {  } {  } 0 0 "Fitter placement was successful" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_PLACEMENT_END" "00:00:00 " "Info: Fitter placement operations ending: elapsed time is 00:00:00" {  } {  } 0 0 "Fitter placement operations ending: elapsed time is %1!s!" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_ROUTING_START" "" "Info: Fitter routing operations beginning" {  } {  } 0 0 "Fitter routing operations beginning" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_VPR_PERCENT_ROUTING_RESOURCE_USAGE" "0 " "Info: Average interconnect usage is 0% of the available device resources" { { "Info" "IFITAPI_FITAPI_VPR_PEAK_ROUTING_REGION" "0 X23_Y0 X34_Y9 " "Info: Peak interconnect usage is 0% of the available device resources in the region that extends from location X23_Y0 to location X34_Y9" {  } {  } 0 0 "Peak interconnect usage is %1!d!%% of the available device resources in the region that extends from location %2!s! to location %3!s!" 0 0 "" 0 -1}  } {  } 0 0 "Average interconnect usage is %1!d!%% of the available device resources" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_VPR_FITTER_ROUTING_END" "00:00:00 " "Info: Fitter routing operations ending: elapsed time is 00:00:00" {  } {  } 0 0 "Fitter routing operations ending: elapsed time is %1!s!" 0 0 "" 0 -1}
{ "Info" "IFITAPI_FITAPI_VPR_AUTO_FIT_ENABLED_AND_USED" "" "Info: The Fitter performed an Auto Fit compilation.  Optimizations were skipped to reduce compilation time." { { "Info" "IFITAPI_FITAPI_VPR_AUTO_FIT_ENABLED_AND_USED_FOR_ROUTABILITY" "" "Info: Optimizations that may affect the design's routability were skipped" {  } {  } 0 0 "Optimizations that may affect the design's routability were skipped" 0 0 "" 0 -1} { "Info" "IFITAPI_FITAPI_VPR_AUTO_FIT_ENABLED_AND_USED_FOR_TIMING" "" "Info: Optimizations that may affect the design's timing were skipped" {  } {  } 0 0 "Optimizations that may affect the design's timing were skipped" 0 0 "" 0 -1}  } {  } 0 0 "The Fitter performed an Auto Fit compilation.  Optimizations were skipped to reduce compilation time." 0 0 "" 0 -1}
{ "Info" "IDAT_DAT_STARTED" "" "Info: Started post-fitting delay annotation" {  } {  } 0 0 "Started post-fitting delay annotation" 0 0 "" 0 -1}
{ "Warning" "WDAT_NO_LOADING_SPECIFIED_ONE_OR_MORE_PINS" "8 " "Warning: Found 8 output pins without output pin load capacitance assignment" { { "Info" "IDAT_NO_LOADING_SPECIFIED_ON_PIN" "Y0 0 " "Info: Pin \"Y0\" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis" {  } {  } 0 0 "Pin \"%1!s!\" has no specified output pin load capacitance -- assuming default load capacitance of %2!d! pF for timing analysis" 0 0 "" 0 -1} { "Info" "IDAT_NO_LOADING_SPECIFIED_ON_PIN" "Y1 0 " "Info: Pin \"Y1\" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis" {  } {  } 0 0 "Pin \"%1!s!\" has no specified output pin load capacitance -- assuming default load capacitance of %2!d! pF for timing analysis" 0 0 "" 0 -1} { "Info" "IDAT_NO_LOADING_SPECIFIED_ON_PIN" "Y2 0 " "Info: Pin \"Y2\" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis" {  } {  } 0 0 "Pin \"%1!s!\" has no specified output pin load capacitance -- assuming default load capacitance of %2!d! pF for timing analysis" 0 0 "" 0 -1} { "Info" "IDAT_NO_LOADING_SPECIFIED_ON_PIN" "Y3 0 " "Info: Pin \"Y3\" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis" {  } {  } 0 0 "Pin \"%1!s!\" has no specified output pin load capacitance -- assuming default load capacitance of %2!d! pF for timing analysis" 0 0 "" 0 -1} { "Info" "IDAT_NO_LOADING_SPECIFIED_ON_PIN" "Y4 0 " "Info: Pin \"Y4\" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis" {  } {  } 0 0 "Pin \"%1!s!\" has no specified output pin load capacitance -- assuming default load capacitance of %2!d! pF for timing analysis" 0 0 "" 0 -1} { "Info" "IDAT_NO_LOADING_SPECIFIED_ON_PIN" "Y5 0 " "Info: Pin \"Y5\" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis" {  } {  } 0 0 "Pin \"%1!s!\" has no specified output pin load capacitance -- assuming default load capacitance of %2!d! pF for timing analysis" 0 0 "" 0 -1} { "Info" "IDAT_NO_LOADING_SPECIFIED_ON_PIN" "Y6 0 " "Info: Pin \"Y6\" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis" {  } {  } 0 0 "Pin \"%1!s!\" has no specified output pin load capacitance -- assuming default load capacitance of %2!d! pF for timing analysis" 0 0 "" 0 -1} { "Info" "IDAT_NO_LOADING_SPECIFIED_ON_PIN" "Y7 0 " "Info: Pin \"Y7\" has no specified output pin load capacitance -- assuming default load capacitance of 0 pF for timing analysis" {  } {  } 0 0 "Pin \"%1!s!\" has no specified output pin load capacitance -- assuming default load capacitance of %2!d! pF for timing analysis" 0 0 "" 0 -1}  } {  } 0 0 "Found %1!d! output pins without output pin load capacitance assignment" 0 0 "" 0 -1}
{ "Info" "IDAT_DAT_COMPLETED" "" "Info: Delay annotation completed successfully" {  } {  } 0 0 "Delay annotation completed successfully" 0 0 "" 0 -1}
{ "Warning" "WFIOMGR_RESERVE_ASSIGNMENT_FOR_UNUSED_PINS_IS_DEFAULT" "As output driving ground " "Warning: The Reserve All Unused Pins setting has not been specified, and will default to 'As output driving ground'." {  } {  } 0 0 "The Reserve All Unused Pins setting has not been specified, and will default to '%1!s!'." 0 0 "" 0 -1}
{ "Info" "IRDB_WROTE_SUPPRESSED_MSGS" "D:/projects/quartus/double_selector_8b/double_selector_8b.fit.smsg " "Info: Generated suppressed messages file D:/projects/quartus/double_selector_8b/double_selector_8b.fit.smsg" {  } {  } 0 0 "Generated suppressed messages file %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Fitter 0 s 2 s Quartus II " "Info: Quartus II Fitter was successful. 0 errors, 2 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "306 " "Info: Peak virtual memory: 306 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Mon Mar 07 11:20:35 2022 " "Info: Processing ended: Mon Mar 07 11:20:35 2022" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:01 " "Info: Elapsed time: 00:00:01" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:01 " "Info: Total CPU time (on all processors): 00:00:01" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Assembler Quartus II " "Info: Running Quartus II Assembler" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition " "Info: Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Mon Mar 07 11:20:35 2022 " "Info: Processing started: Mon Mar 07 11:20:35 2022" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_asm --read_settings_files=off --write_settings_files=off double_selector_8b -c double_selector_8b " "Info: Command: quartus_asm --read_settings_files=off --write_settings_files=off double_selector_8b -c double_selector_8b" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "IASM_ASM_GENERATING_POWER_DATA" "" "Info: Writing out detailed assembly data for power analysis" {  } {  } 0 0 "Writing out detailed assembly data for power analysis" 0 0 "" 0 -1}
{ "Info" "IASM_ASM_GENERATING_PROGRAMMING_FILES" "" "Info: Assembler is generating device programming files" {  } {  } 0 0 "Assembler is generating device programming files" 0 0 "" 0 -1}
{ "Info" "IPGMIO_CONDONE_ERROR_CHECKS_DISABLED" "" "Info: The Active Serial/Parallel mode CONF_DONE pin error check is disabled" {  } {  } 0 0 "The Active Serial/Parallel mode CONF_DONE pin error check is disabled" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Assembler 0 s 0 s Quartus II " "Info: Quartus II Assembler was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "241 " "Info: Peak virtual memory: 241 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Mon Mar 07 11:20:36 2022 " "Info: Processing ended: Mon Mar 07 11:20:36 2022" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:01 " "Info: Elapsed time: 00:00:01" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:00 " "Info: Total CPU time (on all processors): 00:00:00" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Classic Timing Analyzer Quartus II " "Info: Running Quartus II Classic Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition " "Info: Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Mon Mar 07 11:20:37 2022 " "Info: Processing started: Mon Mar 07 11:20:37 2022" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_tan --read_settings_files=off --write_settings_files=off double_selector_8b -c double_selector_8b --timing_analysis_only " "Info: Command: quartus_tan --read_settings_files=off --write_settings_files=off double_selector_8b -c double_selector_8b --timing_analysis_only" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "IQCU_PARALLEL_AUTODETECT_MULTIPLE_PROCESSORS" "4 4 " "Info: Parallel compilation is enabled and will use 4 of the 4 processors detected" {  } {  } 0 0 "Parallel compilation is enabled and will use %1!i! of the %2!i! processors detected" 0 0 "" 0 -1}
{ "Info" "ITDB_FULL_TPD_RESULT" "b6 Y6 14.785 ns Longest " "Info: Longest tpd from source pin \"b6\" to destination pin \"Y6\" is 14.785 ns" { { "Info" "ITDB_NODE_DELAY" "IC(0.000 ns) + CELL(0.974 ns) 0.974 ns b6 1 PIN PIN_75 1 " "Info: 1: + IC(0.000 ns) + CELL(0.974 ns) = 0.974 ns; Loc. = PIN_75; Fanout = 1; PIN Node = 'b6'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "" { b6 } "NODE_NAME" } } { "double_selector_8b.bdf" "" { Schematic "D:/projects/quartus/double_selector_8b/double_selector_8b.bdf" { { 664 64 232 680 "b6" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(6.679 ns) + CELL(0.651 ns) 8.304 ns inst7 2 COMB LCCOMB_X25_Y2_N12 1 " "Info: 2: + IC(6.679 ns) + CELL(0.651 ns) = 8.304 ns; Loc. = LCCOMB_X25_Y2_N12; Fanout = 1; COMB Node = 'inst7'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "7.330 ns" { b6 inst7 } "NODE_NAME" } } { "double_selector_8b.bdf" "" { Schematic "D:/projects/quartus/double_selector_8b/double_selector_8b.bdf" { { 392 664 728 440 "inst7" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(3.365 ns) + CELL(3.116 ns) 14.785 ns Y6 3 PIN PIN_149 0 " "Info: 3: + IC(3.365 ns) + CELL(3.116 ns) = 14.785 ns; Loc. = PIN_149; Fanout = 0; PIN Node = 'Y6'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "6.481 ns" { inst7 Y6 } "NODE_NAME" } } { "double_selector_8b.bdf" "" { Schematic "D:/projects/quartus/double_selector_8b/double_selector_8b.bdf" { { 408 816 992 424 "Y6" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_CELL_DELAY" "4.741 ns ( 32.07 % ) " "Info: Total cell delay = 4.741 ns ( 32.07 % )" {  } {  } 0 0 "Total cell delay = %1!s! %2!s!" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_IC_DELAY" "10.044 ns ( 67.93 % ) " "Info: Total interconnect delay = 10.044 ns ( 67.93 % )" {  } {  } 0 0 "Total interconnect delay = %1!s! %2!s!" 0 0 "" 0 -1}  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "14.785 ns" { b6 inst7 Y6 } "NODE_NAME" } } { "d:/altera/90sp2/quartus/bin/Technology_Viewer.qrui" "" { "TechnologyMapViewer" "d:/altera/90sp2/quartus/bin/Technology_Viewer.qrui" "14.785 ns" { b6 {} b6~combout {} inst7 {} Y6 {} } { 0.000ns 0.000ns 6.679ns 3.365ns } { 0.000ns 0.974ns 0.651ns 3.116ns } "" } }  } 0 0 "%4!s! tpd from source pin \"%1!s!\" to destination pin \"%2!s!\" is %3!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Classic Timing Analyzer 0 s 0 s Quartus II " "Info: Quartus II Classic Timing Analyzer was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "212 " "Info: Peak virtual memory: 212 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Mon Mar 07 11:20:37 2022 " "Info: Processing ended: Mon Mar 07 11:20:37 2022" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:00 " "Info: Elapsed time: 00:00:00" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:00 " "Info: Total CPU time (on all processors): 00:00:00" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
{ "Info" "IFLOW_ERROR_COUNT" "Full Compilation 0 s 2 s " "Info: Quartus II Full Compilation was successful. 0 errors, 2 warnings" {  } {  } 0 0 "Quartus II %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
