{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Classic Timing Analyzer Quartus II " "Info: Running Quartus II Classic Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition " "Info: Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Tue Mar 08 15:17:19 2022 " "Info: Processing started: Tue Mar 08 15:17:19 2022" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_tan --read_settings_files=off --write_settings_files=off shifter_8b -c shifter_8b --timing_analysis_only " "Info: Command: quartus_tan --read_settings_files=off --write_settings_files=off shifter_8b -c shifter_8b --timing_analysis_only" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "IQCU_PARALLEL_AUTODETECT_MULTIPLE_PROCESSORS" "4 4 " "Info: Parallel compilation is enabled and will use 4 of the 4 processors detected" {  } {  } 0 0 "Parallel compilation is enabled and will use %1!i! of the %2!i! processors detected" 0 0 "" 0 -1}
{ "Info" "ITDB_FULL_TPD_RESULT" "LM Y5 15.661 ns Longest " "Info: Longest tpd from source pin \"LM\" to destination pin \"Y5\" is 15.661 ns" { { "Info" "ITDB_NODE_DELAY" "IC(0.000 ns) + CELL(0.994 ns) 0.994 ns LM 1 PIN PIN_69 7 " "Info: 1: + IC(0.000 ns) + CELL(0.994 ns) = 0.994 ns; Loc. = PIN_69; Fanout = 7; PIN Node = 'LM'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "" { LM } "NODE_NAME" } } { "shifter_8b.bdf" "" { Schematic "D:/projects/quartus/shifter_8b/shifter_8b.bdf" { { 456 40 208 472 "LM" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(6.879 ns) + CELL(0.650 ns) 8.523 ns triple_selector_8b:inst\|inst23~0 2 COMB LCCOMB_X26_Y1_N18 1 " "Info: 2: + IC(6.879 ns) + CELL(0.650 ns) = 8.523 ns; Loc. = LCCOMB_X26_Y1_N18; Fanout = 1; COMB Node = 'triple_selector_8b:inst\|inst23~0'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "7.529 ns" { LM triple_selector_8b:inst|inst23~0 } "NODE_NAME" } } { "triple_selector_8b.bdf" "" { Schematic "D:/projects/quartus/shifter_8b/triple_selector_8b.bdf" { { 352 488 552 400 "inst23" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(0.370 ns) + CELL(0.624 ns) 9.517 ns triple_selector_8b:inst\|inst23 3 COMB LCCOMB_X26_Y1_N20 1 " "Info: 3: + IC(0.370 ns) + CELL(0.624 ns) = 9.517 ns; Loc. = LCCOMB_X26_Y1_N20; Fanout = 1; COMB Node = 'triple_selector_8b:inst\|inst23'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "0.994 ns" { triple_selector_8b:inst|inst23~0 triple_selector_8b:inst|inst23 } "NODE_NAME" } } { "triple_selector_8b.bdf" "" { Schematic "D:/projects/quartus/shifter_8b/triple_selector_8b.bdf" { { 352 488 552 400 "inst23" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(3.028 ns) + CELL(3.116 ns) 15.661 ns Y5 4 PIN PIN_147 0 " "Info: 4: + IC(3.028 ns) + CELL(3.116 ns) = 15.661 ns; Loc. = PIN_147; Fanout = 0; PIN Node = 'Y5'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "6.144 ns" { triple_selector_8b:inst|inst23 Y5 } "NODE_NAME" } } { "shifter_8b.bdf" "" { Schematic "D:/projects/quartus/shifter_8b/shifter_8b.bdf" { { 88 688 864 104 "Y5" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_CELL_DELAY" "5.384 ns ( 34.38 % ) " "Info: Total cell delay = 5.384 ns ( 34.38 % )" {  } {  } 0 0 "Total cell delay = %1!s! %2!s!" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_IC_DELAY" "10.277 ns ( 65.62 % ) " "Info: Total interconnect delay = 10.277 ns ( 65.62 % )" {  } {  } 0 0 "Total interconnect delay = %1!s! %2!s!" 0 0 "" 0 -1}  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "15.661 ns" { LM triple_selector_8b:inst|inst23~0 triple_selector_8b:inst|inst23 Y5 } "NODE_NAME" } } { "d:/altera/90sp2/quartus/bin/Technology_Viewer.qrui" "" { "TechnologyMapViewer" "d:/altera/90sp2/quartus/bin/Technology_Viewer.qrui" "15.661 ns" { LM {} LM~combout {} triple_selector_8b:inst|inst23~0 {} triple_selector_8b:inst|inst23 {} Y5 {} } { 0.000ns 0.000ns 6.879ns 0.370ns 3.028ns } { 0.000ns 0.994ns 0.650ns 0.624ns 3.116ns } "" } }  } 0 0 "%4!s! tpd from source pin \"%1!s!\" to destination pin \"%2!s!\" is %3!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Classic Timing Analyzer 0 s 0 s Quartus II " "Info: Quartus II Classic Timing Analyzer was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "212 " "Info: Peak virtual memory: 212 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Tue Mar 08 15:17:19 2022 " "Info: Processing ended: Tue Mar 08 15:17:19 2022" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:00 " "Info: Elapsed time: 00:00:00" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:00 " "Info: Total CPU time (on all processors): 00:00:00" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
