{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Classic Timing Analyzer Quartus II " "Info: Running Quartus II Classic Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition " "Info: Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Mon Mar 07 09:13:08 2022 " "Info: Processing started: Mon Mar 07 09:13:08 2022" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_tan --read_settings_files=off --write_settings_files=off 38_decoder -c 38_decoder --timing_analysis_only " "Info: Command: quartus_tan --read_settings_files=off --write_settings_files=off 38_decoder -c 38_decoder --timing_analysis_only" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "IQCU_PARALLEL_AUTODETECT_MULTIPLE_PROCESSORS" "4 4 " "Info: Parallel compilation is enabled and will use 4 of the 4 processors detected" {  } {  } 0 0 "Parallel compilation is enabled and will use %1!i! of the %2!i! processors detected" 0 0 "" 0 -1}
{ "Info" "ITDB_FULL_TPD_RESULT" "I2 Y2 13.383 ns Longest " "Info: Longest tpd from source pin \"I2\" to destination pin \"Y2\" is 13.383 ns" { { "Info" "ITDB_NODE_DELAY" "IC(0.000 ns) + CELL(0.995 ns) 0.995 ns I2 1 PIN PIN_41 8 " "Info: 1: + IC(0.000 ns) + CELL(0.995 ns) = 0.995 ns; Loc. = PIN_41; Fanout = 8; PIN Node = 'I2'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "" { I2 } "NODE_NAME" } } { "38_decoder.bdf" "" { Schematic "D:/projects/quartus/38_decoder/38_decoder.bdf" { { 144 32 200 160 "I2" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(5.786 ns) + CELL(0.499 ns) 7.280 ns inst10~3 2 COMB LCCOMB_X1_Y7_N22 1 " "Info: 2: + IC(5.786 ns) + CELL(0.499 ns) = 7.280 ns; Loc. = LCCOMB_X1_Y7_N22; Fanout = 1; COMB Node = 'inst10~3'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "6.285 ns" { I2 inst10~3 } "NODE_NAME" } } { "38_decoder.bdf" "" { Schematic "D:/projects/quartus/38_decoder/38_decoder.bdf" { { 360 544 608 408 "inst10" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(2.847 ns) + CELL(3.256 ns) 13.383 ns Y2 3 PIN PIN_195 0 " "Info: 3: + IC(2.847 ns) + CELL(3.256 ns) = 13.383 ns; Loc. = PIN_195; Fanout = 0; PIN Node = 'Y2'" {  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "6.103 ns" { inst10~3 Y2 } "NODE_NAME" } } { "38_decoder.bdf" "" { Schematic "D:/projects/quartus/38_decoder/38_decoder.bdf" { { 280 664 840 296 "Y2" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_CELL_DELAY" "4.750 ns ( 35.49 % ) " "Info: Total cell delay = 4.750 ns ( 35.49 % )" {  } {  } 0 0 "Total cell delay = %1!s! %2!s!" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_IC_DELAY" "8.633 ns ( 64.51 % ) " "Info: Total interconnect delay = 8.633 ns ( 64.51 % )" {  } {  } 0 0 "Total interconnect delay = %1!s! %2!s!" 0 0 "" 0 -1}  } { { "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "d:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "13.383 ns" { I2 inst10~3 Y2 } "NODE_NAME" } } { "d:/altera/90sp2/quartus/bin/Technology_Viewer.qrui" "" { "TechnologyMapViewer" "d:/altera/90sp2/quartus/bin/Technology_Viewer.qrui" "13.383 ns" { I2 {} I2~combout {} inst10~3 {} Y2 {} } { 0.000ns 0.000ns 5.786ns 2.847ns } { 0.000ns 0.995ns 0.499ns 3.256ns } "" } }  } 0 0 "%4!s! tpd from source pin \"%1!s!\" to destination pin \"%2!s!\" is %3!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Classic Timing Analyzer 0 s 0 s Quartus II " "Info: Quartus II Classic Timing Analyzer was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "212 " "Info: Peak virtual memory: 212 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Mon Mar 07 09:13:08 2022 " "Info: Processing ended: Mon Mar 07 09:13:08 2022" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:00 " "Info: Elapsed time: 00:00:00" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:00 " "Info: Total CPU time (on all processors): 00:00:00" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
