{ "Info" "IQEXE_SEPARATOR" "" "Info: *******************************************************************" {  } {  } 3 0 "*******************************************************************" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_PRODUCT" "Classic Timing Analyzer Quartus II " "Info: Running Quartus II Classic Timing Analyzer" { { "Info" "IQEXE_START_BANNER_VERSION" "Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition " "Info: Version 9.0 Build 235 06/17/2009 Service Pack 2 SJ Web Edition" {  } {  } 0 0 "%1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_START_BANNER_TIME" "Mon Mar 07 11:15:57 2022 " "Info: Processing started: Mon Mar 07 11:15:57 2022" {  } {  } 0 0 "Processing started: %1!s!" 0 0 "" 0 -1}  } {  } 4 0 "Running %2!s! %1!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_START_BANNER_COMMANDLINE" "quartus_tan --read_settings_files=off --write_settings_files=off shifter_8b -c shifter_8b --timing_analysis_only " "Info: Command: quartus_tan --read_settings_files=off --write_settings_files=off shifter_8b -c shifter_8b --timing_analysis_only" {  } {  } 0 0 "Command: %1!s!" 0 0 "" 0 -1}
{ "Info" "IQCU_PARALLEL_AUTODETECT_MULTIPLE_PROCESSORS" "4 6 " "Info: Parallel compilation is enabled and will use 4 of the 6 processors detected" {  } {  } 0 0 "Parallel compilation is enabled and will use %1!i! of the %2!i! processors detected" 0 0 "" 0 -1}
{ "Info" "ITDB_FULL_TPD_RESULT" "A6 Y7 13.413 ns Longest " "Info: Longest tpd from source pin \"A6\" to destination pin \"Y7\" is 13.413 ns" { { "Info" "ITDB_NODE_DELAY" "IC(0.000 ns) + CELL(0.994 ns) 0.994 ns A6 1 PIN PIN_67 3 " "Info: 1: + IC(0.000 ns) + CELL(0.994 ns) = 0.994 ns; Loc. = PIN_67; Fanout = 3; PIN Node = 'A6'" {  } { { "c:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "" { A6 } "NODE_NAME" } } { "shifter_8b.bdf" "" { Schematic "D:/dev/quartus/shifter_8b/shifter_8b.bdf" { { 120 40 208 136 "A6" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(6.895 ns) + CELL(0.624 ns) 8.513 ns triple_selector_8b:inst\|inst31 2 COMB LCCOMB_X1_Y5_N10 1 " "Info: 2: + IC(6.895 ns) + CELL(0.624 ns) = 8.513 ns; Loc. = LCCOMB_X1_Y5_N10; Fanout = 1; COMB Node = 'triple_selector_8b:inst\|inst31'" {  } { { "c:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "7.519 ns" { A6 triple_selector_8b:inst|inst31 } "NODE_NAME" } } { "triple_selector_8b.bdf" "" { Schematic "D:/dev/quartus/shifter_8b/triple_selector_8b.bdf" { { 64 488 552 112 "inst31" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_NODE_DELAY" "IC(1.604 ns) + CELL(3.296 ns) 13.413 ns Y7 3 PIN PIN_60 0 " "Info: 3: + IC(1.604 ns) + CELL(3.296 ns) = 13.413 ns; Loc. = PIN_60; Fanout = 0; PIN Node = 'Y7'" {  } { { "c:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "4.900 ns" { triple_selector_8b:inst|inst31 Y7 } "NODE_NAME" } } { "shifter_8b.bdf" "" { Schematic "D:/dev/quartus/shifter_8b/shifter_8b.bdf" { { 56 688 864 72 "Y7" "" } } } }  } 0 0 "%4!d!: + %1!s! = %2!s!; Loc. = %6!s!; Fanout = %7!d!; %5!s! Node = '%3!s!'" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_CELL_DELAY" "4.914 ns ( 36.64 % ) " "Info: Total cell delay = 4.914 ns ( 36.64 % )" {  } {  } 0 0 "Total cell delay = %1!s! %2!s!" 0 0 "" 0 -1} { "Info" "ITDB_TOTAL_IC_DELAY" "8.499 ns ( 63.36 % ) " "Info: Total interconnect delay = 8.499 ns ( 63.36 % )" {  } {  } 0 0 "Total interconnect delay = %1!s! %2!s!" 0 0 "" 0 -1}  } { { "c:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" { Floorplan "c:/altera/90sp2/quartus/bin/TimingClosureFloorplan.fld" "" "13.413 ns" { A6 triple_selector_8b:inst|inst31 Y7 } "NODE_NAME" } } { "c:/altera/90sp2/quartus/bin/Technology_Viewer.qrui" "" { "TechnologyMapViewer" "c:/altera/90sp2/quartus/bin/Technology_Viewer.qrui" "13.413 ns" { A6 {} A6~combout {} triple_selector_8b:inst|inst31 {} Y7 {} } { 0.000ns 0.000ns 6.895ns 1.604ns } { 0.000ns 0.994ns 0.624ns 3.296ns } "" } }  } 0 0 "%4!s! tpd from source pin \"%1!s!\" to destination pin \"%2!s!\" is %3!s!" 0 0 "" 0 -1}
{ "Info" "IQEXE_ERROR_COUNT" "Classic Timing Analyzer 0 s 0 s Quartus II " "Info: Quartus II Classic Timing Analyzer was successful. 0 errors, 0 warnings" { { "Info" "IQEXE_END_PEAK_VSIZE_MEMORY" "191 " "Info: Peak virtual memory: 191 megabytes" {  } {  } 0 0 "Peak virtual memory: %1!s! megabytes" 0 0 "" 0 -1} { "Info" "IQEXE_END_BANNER_TIME" "Mon Mar 07 11:15:58 2022 " "Info: Processing ended: Mon Mar 07 11:15:58 2022" {  } {  } 0 0 "Processing ended: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_TIME" "00:00:01 " "Info: Elapsed time: 00:00:01" {  } {  } 0 0 "Elapsed time: %1!s!" 0 0 "" 0 -1} { "Info" "IQEXE_ELAPSED_CPU_TIME" "00:00:00 " "Info: Total CPU time (on all processors): 00:00:00" {  } {  } 0 0 "Total CPU time (on all processors): %1!s!" 0 0 "" 0 -1}  } {  } 0 0 "%6!s! %1!s! was successful. %2!d! error%3!s!, %4!d! warning%5!s!" 0 0 "" 0 -1}
